🔧 Governance Scaffold – v1.2 (Hybrid + SAVE\_CONFIG)

Generated: 2025-08-18 23:53

# Phases

• P0 – Baseline: restore clean `printer.cfg`; ensure a single SAVE\_CONFIG block at tail; add includes at top.

• P1 – Canary: include only one macro in `governance\_macros.canary.cfg`; restart; run once.

• P2 – Promote: move passing macro into `governance\_macros.promoted.cfg`; tag in Git.

• P3 – Mass Edit (optional): only after PROMOTE + diff preview and operator approval.

• P4 – Rollback: use Git tag or checkpoint; never edit below SAVE\_CONFIG marker.

# Checklists

RESPOND: MSG only, no semicolons/[], indent under gcode.

Mesh: avoid 'default'; use code→name mapping; set hydration flag after saving.

Delta: finish factory calibration once before governance automation.

SAVE\_CONFIG: one marker only; nothing below it besides auto‑generated content.